{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["封面","第1页"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"封面","index":0,"n_rows":20,"n_cols":3,"rows_kept":20,"merged":[[5,1,5,8],[6,2,6,7]],"flags":["formulas_cached_only"]}
[]
[]
[]
[]
[]
[null,"无锡市第一中学信息中心装饰工程"]
[null,null,"分部分项工程量清单与报价表"]
{"$rows_empty":10}
[null,null,"报价单位："]
[]
[null,null,"报价时间："]

{"sheet":"第1页","index":1,"n_rows":57,"n_cols":9,"rows_kept":57,"merged":[[0,0,1,8],[2,0,2,8],[3,0,4,0],[3,1,4,1],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,3,8],[5,2,5,3],[21,2,21,3],[22,2,22,3],[23,0,23,6],[26,2,26,3],[54,0,54,6],[55,0,55,6],[56,0,56,8]],"flags":["formulas_cached_only"]}
["分部分项工程量清单与计价表"]
[]
["工程名称:控制机房及实验教室装饰工程                        标段:"]
["序号","项目编码","项目名称","项目特征描述","计量\r\n单位","工程量","金   额(元)"]
[{"$nulls":6},"综合单价","合价","其中：\r\n暂估价"]
["",null,"（）机房装饰工程",null,null,0,0,0,0]
["1","BB001","拆除顶棚工程","1.拆除原有硅钙扳面层，并要小心拆好运到楼上实验教重新利用\r\n2.拆除龙骨支架及垃圾运下去汽车外运掉","M2",{"v":85,"d":"85.000"},0,0,0]
["2","030213004001","格栅光灯拆除","1.拆除600方格栅日光灯\r\n2.拆下来的灯具搬运到甲方创库堆放好\r","套",{"v":20,"d":"20.000"},0,0,0]
["3","BB002","拆除原有600*600静电地板","1拆除原有静电地板，\r\n2.并搬运到5楼堆放好\r\n","M2",{"v":86.5,"d":"86.500"},0,0,0]
["4","020302001001","天棚吊顶","1.吊顶轻钢龙骨支架\r\n2.600*600*1.0厚铝扣板面层\r,白色，无孔","m2",{"v":86.5,"d":"86.500"},0,0,0]
["5","020209001001","隔断","1.12MM玻璃隔墙用冷轧板底座及顶座基础\r","M",{"v":20.6,"d":"20.600"},0,0,0]
["6","020209001002","隔断","1.12MM玻璃隔墙用冷轧板框子基础\r","M",{"v":17,"d":"17.000"},0,0,0]
["7","020209001003","隔断","1.12MM钢化玻璃隔墙安装\r","M2",{"v":32,"d":"32.000"},0,0,0]
["8","020209001004","隔断","1.四框座两边304不锈钢板1.0厚包边安装\r","M",{"v":55,"d":"55.000"},0,0,0]
["9","020506001001","防尘油漆环氧地坪","1.刷底除一遍满批环氧腻子二遍\r\n2.中涂一遍、面涂二遍\r","m2",{"v":86,"d":"86.000"},0,0,0]
["10","020404006001","全玻自由门（无扇框）","1.无框12MM厚钢化玻璃\r\n2.地弹簧用品牌GMT\r","樘",{"v":1,"d":"1.000"},0,0,0]
["11","030213004002","格栅光灯安装","1.安装600方亚光铝格栅日光灯用品牌（飞利浦、雷仕、松下）\r","套",{"v":20,"d":"20.000"},0,0,0]
["12","020104003001","防静电活动地板","1.铺设600方抗静电地板\r\n2.静电地板到五搂搬运下来有甲供\r","m2",{"v":86,"d":"86.000"},0,0,0]
["13","020408004001","窗帘","1.安装加厚遮光窗帘布\r(卷帘)","M2",{"v":21.07,"d":"21.070"},0,0,0]
["14","BB003","材料上搂、垃圾外运","1.整亇装饰材料搬运到4搂\r\n2.整亇建筑垃圾外运掉\r","项",{"v":1,"d":"1.000"},0,0,0]
["15","BB003","材料上搂、外运","1.室内部分贵重物品、设备搬运\r","项",{"v":1,"d":"1.000"}]
[null,null,"分部小计",null,null,0,0,0,0]
[null,null,"（2）实验教室装饰",null,null,0,0,0,0]
["本页小计",{"$nulls":6},0,0]
["19","020104003002","防静电活动地板","1.拆除原有抗静电地板 2.铺设600方抗静电地板\r\n3.电板利用机房拆下的旧的静电地板\r","m2",{"v":100,"d":"100.000"},0,0,0]
["22","030213004002","安装空气开关","1.安装施耐德断路器 DPN16A双进双出 Acti9 IC65N","只",{"v":12,"d":"12.000"},0,0,0]
[null,null,"分部小计",null,null,0,0,0,0]
{"$rows_empty":27}
["本页小计",{"$nulls":6},0,0]
["合   计",{"$nulls":6},0,0]
["【新点2008清单造价江苏版 V9.2.20】"]